Project 9-Quad Copter downloading IMU from RPi to Host via Bluetooth

Using the IMU connected to the Arduino, mounted on the QuadCopter and [hopefully] flying, capture Roll+Pitch+Yaw, send via Serial over USB to the RPi, send via Bluetooth from RPi to your Host, and display on your Host.

Submit per directions in “Project Submission.docx”